TRUE PARTNERS SUPPLEMENTARY AC CALCULATOR |  |  |  |  |  |  |
Occupancy |  | People |  |  |  |  |  |
Area |  | sqm |  |  |  |  |  |
B/B Occupancy |  | sqm/person |  |  |  |  |  |
B/B Outside-air allowance |  | L/s/person |  |  |  |  |  |
B/B Outside-air allowance |  | L/s |  |  |  |  |
Number of PPL over BB allowance |  |  |  |  |  |  |
Fitout outside-air requirement (G4 Filter) |  | L/s/person |  |  |  |  |  |
Supp. OA to be provided (G4 Filter) |  | L/s |  |  |  |  |  |
Overall O/A L/s (BB+ Supp) |  | L/s |  |  |  |  |  |
Location: |  | (degC) |  |  |  |  |  |
Outside summer DB |  |  |  |  |  |  |  |
Outside summer CWB |  |  |  |  |  |  |  |
HR(g/kg) |  |  |  |  |  |  |  |
Outside winter temp |  |  |  |  |  |  |  |
Space design temp |  |  |  |  |  |  |  |
HR(g/kg) |  |  |  |  |  |  |  |
Safety factor |  |  |  |  |  |  |  |
People Load |  |  |  |  |  |  |  |
Activity: |  |  |  |  |  |  |  |
| Watts/PP |  |  |  |  |  |  |
People Sensible |  |  |  |  |  |  |  |
People Latent |  |  |  |  |  |  |  |
People Overall |  |  |  |  |  |  |  |
Ventilation Load without filtration |  |  |  |  |  |  |  |
Clg Sensible |  |  | WATTS |  |  |  |  |
Clg Latent |  |  | WATTS |  |  |  |  |
Clg Overall |  |  | WATTS |  |  |  |  |
Htg Sensible |  |  | WATTS |  |  |  |  |
| Watts/PP |  |  |  |  |  |  |
Electrical load |  |  | WATTS |  |  |  |  |
Additional Electrical Load |  |  | WATTS |  |  |  |  |
Filtration Requirement |  |  |  |  |  |  |  |
| L/s/person of O/A for Supp. AC Unit |  |  |  |  |  |
| Required efficiency |  | % |  |  |  |  |
| Reduced outside-air to |  | L/s |  |  |  |  |
| Filter Eff. Required |  | F4 filter is not available in the market |  |  |  |
Ventilation Load after filtration |  |  |  |  |  |  |  |
Clg Sensible |  | WATTS |  |  |  |  |  |
Clg Latent |  | WATTS |  |  |  |  |  |
Clg Overall |  | WATTS |  |  |  |  |  |
Htg Sensible |  | WATTS |  |  |  |  |  |
SUPPLEMENTARY UNIT SELECTION |  |  |  |
Supply Air |  | L/s |  | L/s |  |  |  |
Outside Air |  | L/s |  | L/s |  |  |  |
Total Clg Capacity |  | kW |  | kW |  |  |  |
Sensible Clg Capacity |  | kW |  | kW |  |  |  |
# units selected |  |  |  |  |  |  |  |
WPAC Selection |  |  |  |  |  |  |  |
CW Flow |  | L/s |  | L/s |  |  |  |
Htg Capacity |  | kW |  | kW |  |  |  |
CASE BREAKOUT + RETURN AIR SPL |  | dB(A) |  | dB(A) |  |  |  |
CASE BREAKOUT + RETURN AIR SWL dB(A) |  | dB(A) |  | dB(A) |  |  |  |
Power Source |  |  |  |  |  |  |  |
CE version- Running Current |  | (A) |  | (A) |  |  |  |
CE version- Max. Running Current |  | (A) |  | (A) |  |  |  |
R version- Running Current |  | (A) |  | (A) |  |  |  |
R version- Max. Running Current |  | (A) |  | (A) |  |  |  |
Coil Water side PD |  | (kPa) |  | (kPa) |  |  |  |
Weight - incl. water |  | (kg) |  | (kg) |  |  |  |
EER |  |  |  |  |  |  |  |
COP |  |  |  |  |  |  |  |
Summer Air-on DB |  | degC |  | degC |  |  |  |
Summer Air-on CWB |  | degC |  | degC |  |  |  |
Winter Air-on |  | degC |  | degC |  |  |  |

#### Print All Information

Please host the converted page in server to use Print All.

#### Evaluation only

The page is only for evaluating SpreadsheetConverter
The page as a whole or parts of it is only allowed to be used for evaluating SpreadsheetConverter. All publishing on a webserver, for other purposes than evaluation, requires a license of SpreadsheetConverter.
Do not show next time