TRUE PARTNERS SUPPLEMENTARY AC CALCULATOR
Occupancy |  | People
Area |  | sqm
B/B Occupancy |  | sqm/person
B/B Outside-air allowance |  | L/s/person
B/B Outside-air allowance |  | L/s
Number of PPL over BB allowance |
Fitout outside-air requirement (G4 Filter) |  | L/s/person
Supp. OA to be provided (G4 Filter) |  | L/s
Overall O/A L/s (BB+ Supp) |  | L/s
Location: |  | (degC)
Outside summer DB |
Outside summer CWB |
HR(g/kg) |
Outside winter temp |
Space design temp |
HR(g/kg) |
Safety factor |
People Load
Activity: |
| Watts/PP
People Sensible |  |  | WATTS
People Latent |  |  | WATTS
People Overall |  |  | WATTS
Outside Air Load without filtration
Clg Sensible |  | WATTS
Clg Latent |  | WATTS
Clg Overall |  | WATTS
Htg Sensible |  | WATTS
| Watts/PP
Electrical load |  |  | WATTS
Additional Electrical Load |  |  | WATTS
Filtration Requirement
| L/s/person of O/A for Supp. AC Unit
Required efficiency |  | %
Reduced outside-air to |  | L/s
| Filter Eff. Required |  | F4 filter is not available in the market
Outside Air Load after filtration
Clg Sensible |  | WATTS
Clg Latent |  | WATTS
Clg Overall |  | WATTS
Htg Sensible |  | WATTS
SUPPLEMENTARY UNIT SELECTION
Supply Air |  | L/s |  | L/s
Outside Air |  | L/s |  | L/s
Total Clg Capacity |  | kW |  | kW
Sensible Clg Capacity |  | kW |  | kW
# units selected |  |  |
WPAC Selection |  |  |
CW Flow |  | L/s |  | L/s
Htg Capacity |  | kW |  | kW
CASE BREAKOUT + RETURN AIR SPL |  | dB(A) |  | dB(A)
CASE BREAKOUT + RETURN AIR SWL dB(A) |  | dB(A) |  | dB(A)
Power Source |  |  |
CE version- Running Current |  | (A) |  | (A)
CE version- Max. Running Current |  | (A) |  | (A)
R version- Running Current |  | (A) |  | (A)
R version- Max. Running Current |  | (A) |  | (A)
Coil Water side PD |  | (kPa) |  | (kPa)
Weight - incl. water |  | (kg) |  | (kg)
EER |  |  |
COP |  |  |
Summer Air-on DB |  | degC |  | degC
Summer Air-on CWB |  | degC |  | degC
Winter Air-on |  | degC |  | degC